**REFERENCES**

1. ASTM International Standard Specification for Wrought iron-cobalt high magnetic saturation alloys UNS R 30005 and R 92650, ASTM A 801/A 801M-1999.
2. Technical Data Sheet 4b, Telecon Metals Limited on Permendur 49 .
3. Technical Data Sheet of Soft Magnetic Materials, Vacoflux 50.
4. Product Brochure of M/s Mishra Dhatu Nigam Limited, Hyderabad, India
5. High temperature metals 800-500-2141-permendur 2 V Hiperco 50 A, Technical information (Pp 1 to 4).
6. Development type test schedule for SOFTCOMAG 49AA for forged and hot rolled bars, No. RCMA (M)/90, 2002.
7. Emile Josso Fe-Co-V alloys: A critical study of the phase diagrams in relation to Magnetic properties, IEEE Transactions on Magnetics, Vol.Mag-10, No.2, Pp 161-165, June, 1974.
8. Lesile L. Harner, A simplified method of selecting soft magnetic alloys, May 1999.
9. Richard M. Bozorth, Ferromagnetism, D. Van Nostand Company, Inc., New York, USA.
10. ASTM International Standard test methods for chemical analysis of High-Temperature, Electrical, Magnetic and other similar Iron, Nickel and Cobalt alloys- ASTM E 354-1993.
11. ASTM International: Standard test methods for determination of Carbon, Sulphur, Nitrogen and oxygen in steel and in Iron, Nickel and Cobalt alloys, ASTM E 1019-2003.
12. ASTM International Standard Test Method for Macroetch Testing of Consumable Electrode Remelted Steel Bars and Billets, ASTM A 604-2007.

13. ASTM International Standard test methods for determining average grain size of metals, ASTM E 112-1996.

14. ASTM International Standard test methods for determining the inclusion content of steel, ASTM E 45-1997.

15. ASTM International Standard test method for linear thermal expansion of solid materials with a push-rod dilatometer, ASTM E 228-1995.

16. ASTM International Standard Test Method for Direct-Current Magnetic Properties of Materials Using the Ballistic Method and Ring Specimens, ASTM A 596-1995.

17. ASTM International Standard Test Method for Vickers Hardness of Metallic Materials, ASTM E 92-1997.

18. ASTM International Standard Test Method For Tension Testing Of Metallic Materials, ASTM E 8-2004.

19. ASTM International Standard Test Methods for Elevated Temperature Tension Tests of Metallic Materials, ASTM E29-2008

20. ASTM International Standard Test Method for Young's Modulus, Tangent Modulus, and Chord Modulus, ASTM E111-1997

21. Aeronautical Material Specification for Inspection, Ultrasonic Product Over 0.5 Inch (12.7 mm) Thick, AMS 2630.

22. Aeronautical Material Specification for Tolerances Corrosion and Heat Resistant Steel, Iron Alloy, Titanium, and Titanium Alloy Bars and Wire, AMS 2241.

23. Aeronautical Material Specification for Chemical check analysis limits, corrosion resistant and heat resistant steels and alloys, Maraging and other highly alloyed steels, and Iron alloys, AMS 2248.